Task 6.6

Q1 What ISO/OSI layers does a packet filter usually inspect?

Answer: Layer 3 and 4

Q2 What method can NOT be used during a TLS connection establishment (to an HTTPS webserver)?

Answer: RADIUS

Q3 Which key(s) belong into an X.509 certificate?

Answer: The public key

Q4 Consider you want to connect to a LAN that has 802.1X-controlled ports. What traffic is allowed to pass before a successful authentication?

Answer: EAPoL