Task 5.2

Which hosts of the SecLab are involved in the authentication process? What is the role of each of these hosts in the course of the RADIUS authentication process?

* Hellgate (10.0.0.1) -> User
* White (10.0.0.5) -> RADIUS Client
* Orange (10.0.0.10) -> RADIUS Server

Draw a simple sketch of the hosts and the communication between them using the correct RADIUS nomenclature!

